{"text_format":"3","workbook":"xlsx","n_sheets":14,"sheets":["内部結露計算シート","計算例-1","計算例-2","解説","北海道","東北（青森、岩手、宮城、秋田、山形、福島）","南関東（埼玉、千葉、東京、神奈川）","北関東・甲信（茨城、栃木、群馬、山梨、長野）","北陸（新潟、富山、石川、福井）","東海（岐阜、静岡、愛知、三重）","近畿（滋賀、京都、大阪、兵庫、奈良、和歌山）","中国（鳥取、島根、岡山、広島、山口）","四国（徳島、香川、愛媛、高知）","九州（福岡、佐賀、長崎、熊本、大分、宮崎、鹿児島、沖縄）"],"not_rendered":{"images":41,"defined_names":13},"read":"whole","date_system":"1900"}

{"sheet":"内部結露計算シート","index":0,"n_rows":47,"n_cols":29,"rows_kept":47,"merged":[[1,24,2,24],[2,0,2,1],[2,2,2,5],[2,7,2,9],[4,0,4,1],[4,2,4,3],[4,5,4,6],[5,0,5,1],[6,0,6,1],[7,2,7,6],[9,0,11,2],[9,3,9,4],[9,10,11,10],[9,11,10,12],[9,13,10,14],[9,15,10,17],[9,18,10,19],[11,11,11,12],[11,13,11,14],[11,15,11,17],[12,0,13,2],[12,3,13,3],[12,4,13,4],[12,5,13,5],[12,6,13,6],[12,7,13,7],[12,8,13,8],[12,16,12,17],[13,10,14,10],[13,16,13,17],[14,0,15,0],[14,1,15,2],[14,16,14,17],[15,10,16,10],[15,16,15,17],[16,0,17,0],[16,1,17,2],[16,16,16,17],[17,10,18,10],[17,16,17,17],[18,0,19,0],[18,1,19,2],[18,16,18,17],[19,10,20,10],[19,16,19,17],[20,0,21,0],[20,1,21,2],[20,16,20,17],[21,10,22,10],[21,16,21,17],[22,0,23,0],[22,1,23,2],[22,16,22,17],[23,10,24,10],[23,16,23,17],[24,0,25,0],[24,1,25,2],[24,16,24,17],[25,10,26,10],[25,16,25,17],[26,0,27,0],[26,1,27,2],[26,16,26,17],[27,10,28,10],[27,16,27,17],[28,0,29,0],[28,1,29,2],[28,16,28,17],[29,10,30,10],[29,16,29,17],[30,0,31,0],[30,1,31,2],[30,16,30,17],[31,10,32,10],[31,16,31,17],[32,0,33,0],[32,1,33,2],[32,16,32,17],[33,10,34,10],[33,16,33,17],[34,0,35,0],[34,1,35,2],[34,16,34,17],[35,10,36,10],[35,16,35,17],[36,0,37,0],[36,1,37,2],[36,16,36,17],[37,10,38,10],[37,16,37,17],[38,0,39,2],[38,3,39,3],[38,4,39,4],[38,5,39,5],[38,6,39,6],[38,7,39,7],[38,8,39,8],[38,16,38,17],[39,16,39,17],[40,0,40,2],[41,6,43,19]]}
["内部結露計算シート",{"$nulls":18},"Copy right ⓒ2022　hyoukakyoukai.All right reserved.",{"$nulls":3},"対象部位のリスト"]
[{"$nulls":19},"ver2.0",{"$nulls":4},"室内側表面熱伝達抵抗","室外側表面熱伝達抵抗"]
["物件名",{"$nulls":5},"対象部位",{"$nulls":3},"☜ 計算対象部位を選択",{"$nulls":14},"外気","外気以外"]
["１）室内外条件表",{"$nulls":22},"屋根",0.09,0.04,0.09]
["室内外",null,"温度（℃）",null,"湿度（％）","表面熱伝達抵抗（㎡K/W）",{"$nulls":17},"天井",0.09,"-",0.09]
["室内",null,"ti 　= ",15,60,"Rsi=",{"$f":"IF(H3=X10,\"\",IF(H3=X11,Y11,IF(H3=X12,Y12,IF(H3=X13,Y13,IF(H3=X14,Y14,IF(H3=X16,Y16,IF(H3=X17,Y17,IF(H3=X15,Y15,IF(H3=X18,Y18,falese)))))))))","v":""},{"$nulls":16},"小屋裏に接する断熱壁",0.11,0.11,"-"]
["外気",null,"to※ =",null,70,"Rse=",{"$f":"IF(H3=X10,\"\",IF(H3=X11,Z11,IF(H3=X12,Z12,IF(H3=X13,Z13,IF(H3=X14,Z14,IF(H3=X16,Z16,IF(H3=X17,Z17,IF(H3=X15,Z15,IF(H3=X18,Z18,FALSE)))))))))","v":""},{"$nulls":16},"外壁",0.11,0.04,0.11]
[null,null,"※外気温は建設地の最寒月の平均気温を入力",{"$nulls":20},"床",0.15,0.04,0.15]
["２）層構成物性値一覧表",{"$nulls":9},"３）表面・境界面の温度・水蒸気圧一覧表"]
["材料名 注1",null,null,"厚さ",null,"熱伝導率λ","熱抵抗Ｒ 注2","透湿比抵抗ξ","透湿抵抗Ｒ' 注3",null,null,"温度",null,"飽和水蒸気圧",null,"実在水蒸気圧",null,null,"結露判定"]
[{"$nulls":4},"ｄ","λ＝ｄ÷Ｒ","Ｒ＝ｄ÷λ ","ξ＝Ｒ’÷ｄ","Ｒ’＝ξ×ｄ",{"$nulls":14},"屋根（外気）",0.09,0.04]
[{"$nulls":3},"（mm）","（ｍ）","（W/mK）","（㎡K/W）","（msPa/ng）","（㎡sPa/ng）",null,null,"（℃）",null,"（Pa）",null,"（Pa）",null,null,"fs-fA","判定",{"$nulls":3},"屋根（外気以外・通気層）",0.09,0.09]
["室内",{"$nulls":10},"ti=",{"$f":"IF(D6=\"\",\"\",D6)","v":{"v":15,"d":"15.00"}},"室内fs=",{"$f":"IF(M13=\"\",\"\",IF(M13>=0,100*(POWER(10,-7.90298*(373.16/(M13+273.16)-1)+5.02808*LOG10(373.16/(M13+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M13+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M13+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M13+273.16)-1)-3.56654*LOG10(273.16/(M13+273.16))+0.876793*(1-(M13+273.16)/273.16)+LOG10(6.1071)))))","v":{"v":1704.3783226662495,"d":"1704.38"}},"室内fA=",{"$f":"IF(O13=\"\",\"\",O13*E6*0.01)","v":{"v":1022.6269935997498,"d":"1022.63"}},null,{"$f":"IF(O13=\"\",\"\",O13-Q13)","v":{"v":681.7513290664997,"d":"681.75"}},{"$f":"IF(S13<=0,\"結露\",\"　　\")","v":"　　"},{"$nulls":3},"天井（外気以外・小屋裏）",0.09,0.09]
[{"$nulls":10},"室内表面","θi",null,"fsi",null,"fAi",{"$nulls":7},"外壁（外気）",0.11,0.04]
[1,{"$nulls":11},{"$f":"IF(G6=\"\",\"\",D$6-(D$6-D$7)*G$6/F$43)","v":""},null,{"$f":"IF(M15=\"\",\"\",IF(M15>=0,100*(POWER(10,-7.90298*(373.16/(M15+273.16)-1)+5.02808*LOG10(373.16/(M15+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M15+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M15+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M15+273.16)-1)-3.56654*LOG10(273.16/(M15+273.16))+0.876793*(1-(M15+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"Q13","v":{"v":1022.6269935997498,"d":"1022.63"}},null,{"$f":"IF(O15=\"\",\"\",O15-Q15)","v":""},{"$f":"IF(S15<=0,\"結露\",\"　　\")","v":"　　"},{"$nulls":3},"外壁（外気以外・通気層）",0.11,0.11]
[{"$nulls":4},{"$f":"IF(D16>0,D16/1000,\"\")","v":""},null,{"$f":"IF(F16>0,E16/F16,\"\")","v":""},null,{"$f":"IF(H16>0,H16*E16,\"\")","v":""},null,"1～2 境界面","θ1",null,"fs1",null,"fA1",{"$nulls":7},"小屋裏に接する断熱壁",0.11,0.04]
[2,{"$nulls":11},{"$f":"IF(G16=\"\",\"\",D$6-(D$6-D$7)*(G$6+G16)/F$43)","v":""},null,{"$f":"IF(M17=\"\",\"\",IF(M17>=0,100*(POWER(10,-7.90298*(373.16/(M17+273.16)-1)+5.02808*LOG10(373.16/(M17+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M17+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M17+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M17+273.16)-1)-3.56654*LOG10(273.16/(M17+273.16))+0.876793*(1-(M17+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O17=\"\",\"\",Q$15-(Q$15-Q$40)*I$16/F$44)","v":""},null,{"$f":"IF(O17=\"\",\"\",O17-Q17)","v":""},{"$f":"IF(S17<=0,\"結露\",\"　　\")","v":"　　"},{"$nulls":3},"床（外気）",0.15,0.04]
[{"$nulls":4},{"$f":"IF(D18>0,D18/1000,\"\")","v":""},null,{"$f":"IF(F18>0,E18/F18,\"\")","v":""},null,{"$f":"IF(H18>0,H18*E18,\"\")","v":""},null,"2～3 境界面","θ2",null,"fs2",null,"fA2",{"$nulls":7},"床（外気以外・床裏）",0.15,0.15]
[3,{"$nulls":11},{"$f":"IF(G18=\"\",\"\",D$6-(D$6-D$7)*(G$6+SUM(G16:G18))/F$43)","v":""},null,{"$f":"IF(M19=\"\",\"\",IF(M19>=0,100*(POWER(10,-7.90298*(373.16/(M19+273.16)-1)+5.02808*LOG10(373.16/(M19+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M19+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M19+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M19+273.16)-1)-3.56654*LOG10(273.16/(M19+273.16))+0.876793*(1-(M19+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O19=\"\",\"\",Q$15-(Q$15-Q$40)*SUM(I16:I18)/F$44)","v":""},null,{"$f":"IF(O19=\"\",\"\",O19-Q19)","v":""},{"$f":"IF(S19<=0,\"結露\",\"　　\")","v":"　　"}]
[{"$nulls":4},{"$f":"IF(D20>0,D20/1000,\"\")","v":""},null,{"$f":"IF(F20>0,E20/F20,\"\")","v":""},null,{"$f":"IF(H20>0,H20*E20,\"\")","v":""},null,"3～4 境界面","θ3",null,"fs3",null,"fA3"]
[4,{"$nulls":11},{"$f":"IF(G20=\"\",\"\",D$6-(D$6-D$7)*(G$6+SUM(G16:G20))/F$43)","v":""},null,{"$f":"IF(M21=\"\",\"\",IF(M21>=0,100*(POWER(10,-7.90298*(373.16/(M21+273.16)-1)+5.02808*LOG10(373.16/(M21+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M21+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M21+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M21+273.16)-1)-3.56654*LOG10(273.16/(M21+273.16))+0.876793*(1-(M21+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O21=\"\",\"\",Q$15-(Q$15-Q$40)*SUM(I16:I20)/F$44)","v":""},null,{"$f":"IF(O21=\"\",\"\",O21-Q21)","v":""},{"$f":"IF(S21<=0,\"結露\",\"　　\")","v":"　　"}]
[{"$nulls":4},{"$f":"IF(D22>0,D22/1000,\"\")","v":""},null,{"$f":"IF(F22>0,E22/F22,\"\")","v":""},null,{"$f":"IF(H22>0,H22*E22,\"\")","v":""},null,"4～5 境界面","θ4",null,"fs4",null,"fA4"]
[5,{"$nulls":11},{"$f":"IF(G22=\"\",\"\",D$6-(D$6-D$7)*(G$6+SUM(G16:G22))/F$43)","v":""},null,{"$f":"IF(M23=\"\",\"\",IF(M23>=0,100*(POWER(10,-7.90298*(373.16/(M23+273.16)-1)+5.02808*LOG10(373.16/(M23+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M23+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M23+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M23+273.16)-1)-3.56654*LOG10(273.16/(M23+273.16))+0.876793*(1-(M23+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O23=\"\",\"\",Q$15-(Q$15-Q$40)*SUM(I16:I22)/F$44)","v":""},null,{"$f":"IF(O23=\"\",\"\",O23-Q23)","v":""},{"$f":"IF(S23<=0,\"結露\",\"　　\")","v":"　　"}]
[{"$nulls":4},{"$f":"IF(D24>0,D24/1000,\"\")","v":""},null,{"$f":"IF(F24>0,E24/F24,\"\")","v":""},null,{"$f":"IF(H24>0,H24*E24,\"\")","v":""},null,"5～6 境界面","θ5",null,"fs5",null,"fA5"]
[6,{"$nulls":11},{"$f":"IF(G24=\"\",\"\",D$6-(D$6-D$7)*(G$6+SUM(G16:G24))/F$43)","v":""},null,{"$f":"IF(M25=\"\",\"\",IF(M25>=0,100*(POWER(10,-7.90298*(373.16/(M25+273.16)-1)+5.02808*LOG10(373.16/(M25+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M25+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M25+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M25+273.16)-1)-3.56654*LOG10(273.16/(M25+273.16))+0.876793*(1-(M25+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O25=\"\",\"\",Q$15-(Q$15-Q$40)*SUM(I16:I24)/F$44)","v":""},null,{"$f":"IF(O25=\"\",\"\",O25-Q25)","v":""},{"$f":"IF(S25<=0,\"結露\",\"　　\")","v":"　　"}]
[{"$nulls":4},{"$f":"IF(D26>0,D26/1000,\"\")","v":""},null,{"$f":"IF(F26>0,E26/F26,\"\")","v":""},null,{"$f":"IF(H26>0,H26*E26,\"\")","v":""},null,"6～7 境界面","θ6",null,"fs6",null,"fA6"]
[7,{"$nulls":11},{"$f":"IF(G26=\"\",\"\",D$6-(D$6-D$7)*(G$6+SUM(G16:G26))/F$43)","v":""},null,{"$f":"IF(M27=\"\",\"\",IF(M27>=0,100*(POWER(10,-7.90298*(373.16/(M27+273.16)-1)+5.02808*LOG10(373.16/(M27+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M27+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M27+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M27+273.16)-1)-3.56654*LOG10(273.16/(M27+273.16))+0.876793*(1-(M27+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O27=\"\",\"\",Q$15-(Q$15-Q$40)*SUM(I16:I26)/F$44)","v":""},null,{"$f":"IF(O27=\"\",\"\",O27-Q27)","v":""},{"$f":"IF(S27<=0,\"結露\",\"　　\")","v":"　　"}]
[{"$nulls":4},{"$f":"IF(D28>0,D28/1000,\"\")","v":""},null,{"$f":"IF(F28>0,E28/F28,\"\")","v":""},null,{"$f":"IF(H28>0,H28*E28,\"\")","v":""},null,"7～8 境界面","θ7",null,"fs7",null,"fA7"]
[8,{"$nulls":11},{"$f":"IF(G28=\"\",\"\",D$6-(D$6-D$7)*(G$6+SUM(G16:G28))/F$43)","v":""},null,{"$f":"IF(M29=\"\",\"\",IF(M29>=0,100*(POWER(10,-7.90298*(373.16/(M29+273.16)-1)+5.02808*LOG10(373.16/(M29+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M29+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M29+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M29+273.16)-1)-3.56654*LOG10(273.16/(M29+273.16))+0.876793*(1-(M29+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O29=\"\",\"\",Q$15-(Q$15-Q$40)*SUM(I16:I28)/F$44)","v":""},null,{"$f":"IF(O29=\"\",\"\",O29-Q29)","v":""},{"$f":"IF(S29<=0,\"結露\",\"　　\")","v":"　　"}]
[{"$nulls":4},{"$f":"IF(D30>0,D30/1000,\"\")","v":""},null,{"$f":"IF(F30>0,E30/F30,\"\")","v":""},null,{"$f":"IF(H30>0,H30*E30,\"\")","v":""},null,"8～9 境界面","θ8",null,"fs8",null,"fA8"]
[9,{"$nulls":11},{"$f":"IF(G30=\"\",\"\",D$6-(D$6-D$7)*(G$6+SUM(G16:G30))/F$43)","v":""},null,{"$f":"IF(M31=\"\",\"\",IF(M31>=0,100*(POWER(10,-7.90298*(373.16/(M31+273.16)-1)+5.02808*LOG10(373.16/(M31+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M31+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M31+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M31+273.16)-1)-3.56654*LOG10(273.16/(M31+273.16))+0.876793*(1-(M31+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O31=\"\",\"\",Q$15-(Q$15-Q$40)*SUM(I16:I30)/F$44)","v":""},null,{"$f":"IF(O31=\"\",\"\",O31-Q31)","v":""},{"$f":"IF(S31<=0,\"結露\",\"　　\")","v":"　　"}]
[{"$nulls":4},{"$f":"IF(D32>0,D32/1000,\"\")","v":""},null,{"$f":"IF(F32>0,E32/F32,\"\")","v":""},null,{"$f":"IF(H32>0,H32*E32,\"\")","v":""},null,"9～10 境界面","θ9",null,"fs9",null,"fA9"]
[10,{"$nulls":11},{"$f":"IF(G32=\"\",\"\",D$6-(D$6-D$7)*(G$6+SUM(G16:G32))/F$43)","v":""},null,{"$f":"IF(M33=\"\",\"\",IF(M33>=0,100*(POWER(10,-7.90298*(373.16/(M33+273.16)-1)+5.02808*LOG10(373.16/(M33+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M33+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M33+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M33+273.16)-1)-3.56654*LOG10(273.16/(M33+273.16))+0.876793*(1-(M33+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O33=\"\",\"\",Q$15-(Q$15-Q$40)*SUM(I16:I32)/F$44)","v":""},null,{"$f":"IF(O33=\"\",\"\",O33-Q33)","v":""},{"$f":"IF(S33<=0,\"結露\",\"　　\")","v":"　　"}]
[{"$nulls":4},{"$f":"IF(D34>0,D34/1000,\"\")","v":""},null,{"$f":"IF(F34>0,E34/F34,\"\")","v":""},null,{"$f":"IF(H34>0,H34*E34,\"\")","v":""},null,"10～11 境界面","θ10",null,"fs10",null,"fA10"]
[11,{"$nulls":11},{"$f":"IF(G34=\"\",\"\",D$6-(D$6-D$7)*(G$6+SUM(G16:G34))/F$43)","v":""},null,{"$f":"IF(M35=\"\",\"\",IF(M35>=0,100*(POWER(10,-7.90298*(373.16/(M35+273.16)-1)+5.02808*LOG10(373.16/(M35+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M35+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M35+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M35+273.16)-1)-3.56654*LOG10(273.16/(M35+273.16))+0.876793*(1-(M35+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O35=\"\",\"\",Q$15-(Q$15-Q$40)*SUM(I16:I34)/F$44)","v":""},null,{"$f":"IF(O35=\"\",\"\",O35-Q35)","v":""},{"$f":"IF(S35<=0,\"結露\",\"　　\")","v":"　　"}]
[{"$nulls":4},{"$f":"IF(D36>0,D36/1000,\"\")","v":""},null,{"$f":"IF(F36>0,E36/F36,\"\")","v":""},null,{"$f":"IF(H36>0,H36*E36,\"\")","v":""},null,"11～12 境界面","θ11",null,"fs11",null,"fA11"]
[12,{"$nulls":11},{"$f":"IF(G36=\"\",\"\",D$6-(D$6-D$7)*(G$6+SUM(G16:G36))/F$43)","v":""},null,{"$f":"IF(M37=\"\",\"\",IF(M37>=0,100*(POWER(10,-7.90298*(373.16/(M37+273.16)-1)+5.02808*LOG10(373.16/(M37+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M37+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M37+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M37+273.16)-1)-3.56654*LOG10(273.16/(M37+273.16))+0.876793*(1-(M37+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O37=\"\",\"\",Q$15-(Q$15-Q$40)*SUM(I16:I36)/F$44)","v":""},null,{"$f":"IF(O37=\"\",\"\",O37-Q37)","v":""},{"$f":"IF(S37<=0,\"結露\",\"　　\")","v":"　　"}]
[{"$nulls":4},{"$f":"IF(D38>0,D38/1000,\"\")","v":""},null,{"$f":"IF(F38>0,E38/F38,\"\")","v":""},null,{"$f":"IF(H38>0,H38*E38,\"\")","v":""},null,"外気表面","θO",null,"fso",null,"fAo"]
["外気",{"$nulls":11},{"$f":"IF(ISERROR(D$6-(D$6-D$7)*(G$6+F42)/F$43),\"\",D$6-(D$6-D$7)*(G$6+F42)/F$43)","v":""},null,{"$f":"IF(M39=\"\",\"\",IF(M39>=0,100*(POWER(10,-7.90298*(373.16/(M39+273.16)-1)+5.02808*LOG10(373.16/(M39+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M39+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M39+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M39+273.16)-1)-3.56654*LOG10(273.16/(M39+273.16))+0.876793*(1-(M39+273.16)/273.16)+LOG10(6.1071)))))","v":""},null,{"$f":"IF(O39=\"\",\"\",Q$15-(Q$15-Q$40)*SUM(I16:I38)/F$44)","v":""},null,{"$f":"IF(O39=\"\",\"\",O39-Q39)","v":""},{"$f":"IF(S39<=0,\"結露\",\"　　\")","v":"　　"}]
[{"$nulls":11},"to=",{"$f":"IF(D7=\"\",\"\",D7)","v":""},"外気fs=",{"$f":"IF(M40=\"\",\"\",IF(M40>=0,100*(POWER(10,-7.90298*(373.16/(M40+273.16)-1)+5.02808*LOG10(373.16/(M40+273.16))-1.3816*POWER(10,-7)*(POWER(10,11.344*(1-(M40+273.16)/373.16))-1)+8.1328*POWER(10,-3)*(POWER(10,-3.49149*(373.16/(M40+273.16)-1))-1)+LOG10(1013.246))),100*(POWER(10,-9.09718*(273.16/(M40+273.16)-1)-3.56654*LOG10(273.16/(M40+273.16))+0.876793*(1-(M40+273.16)/273.16)+LOG10(6.1071)))))","v":""},"外気fA=",{"$f":"IF(O40=\"\",\"\",O40*E7*0.01)","v":""},null,{"$f":"IF(O40=\"\",\"\",O40-Q40)","v":""}]
[]
["∑R　熱抵抗合計",null,null,"ΣR",null,{"$f":"SUM(G15:G38)","v":{"v":0,"d":"0.00"}},"　注1：材料の熱伝導率、透湿比抵抗がわからない場合は、厚さ(mm)を1000に設定し熱伝導率、透湿比抵抗の欄に熱抵抗の逆数、透湿抵抗の値を入力する。\n　注2：1）空気層など熱抵抗Rで設定する場合は、厚さ(mm)を1000に設定し熱伝導率λの欄に設定する熱抵抗Rの逆数(1/R）を入力する。\n　　　  2）シート類など、熱性能を無視する場合は、熱伝導率λの欄に10000を入力する。\n　注3：1）防湿層、空気層など透湿抵抗R'で設定する場合は、厚さ(mm)を1000に設定し、透湿比抵抗ξの欄に設定する透湿抵抗R'の値を入力する。"]
[" Rt　熱貫流抵抗",null,null,"Rt＝Ro+ΣR+Ri",null,{"$f":"IF(ISERROR(SUM(G15:G38)+G6+G7),\"\",SUM(G15:G38)+G6+G7)","v":""}]
[" R't　透湿抵抗合計",null,null,"R't＝ΣR'",null,{"$f":"SUM(I15:I38)","v":{"v":0,"d":"0.00"}}]
[]
[]
[{"$nulls":28},1]

{"sheet":"計算例-1","index":1,"n_rows":1,"n_cols":1,"rows_kept":1}
["Excel内部結露計算シートによる計算例-1"]

{"sheet":"計算例-2","index":2,"n_rows":1,"n_cols":1,"rows_kept":1}
["Excel内部結露計算シートによる計算例-2"]

{"sheet":"解説","index":3,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"北海道","index":4,"n_rows":200,"n_cols":10,"rows_kept":200}
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]

{"sheet":"東北（青森、岩手、宮城、秋田、山形、福島）","index":5,"n_rows":160,"n_cols":10,"rows_kept":160}
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]

{"sheet":"南関東（埼玉、千葉、東京、神奈川）","index":6,"n_rows":40,"n_cols":10,"rows_kept":40}
{"$rows_empty":39}
[{"$nulls":9},20220829]

{"sheet":"北関東・甲信（茨城、栃木、群馬、山梨、長野）","index":7,"n_rows":120,"n_cols":10,"rows_kept":120}
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]

{"sheet":"北陸（新潟、富山、石川、福井）","index":8,"n_rows":80,"n_cols":10,"rows_kept":80}
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]

{"sheet":"東海（岐阜、静岡、愛知、三重）","index":9,"n_rows":80,"n_cols":10,"rows_kept":80}
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]

{"sheet":"近畿（滋賀、京都、大阪、兵庫、奈良、和歌山）","index":10,"n_rows":80,"n_cols":10,"rows_kept":80}
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]

{"sheet":"中国（鳥取、島根、岡山、広島、山口）","index":11,"n_rows":80,"n_cols":10,"rows_kept":80}
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]

{"sheet":"四国（徳島、香川、愛媛、高知）","index":12,"n_rows":80,"n_cols":10,"rows_kept":80}
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]

{"sheet":"九州（福岡、佐賀、長崎、熊本、大分、宮崎、鹿児島、沖縄）","index":13,"n_rows":160,"n_cols":10,"rows_kept":160}
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]
{"$rows_empty":39}
[{"$nulls":9},20220829]